--altsyncram ADDRESS_ACLR_A="NONE" ADDRESS_ACLR_B="NONE" ADDRESS_REG_B="CLOCK1" CYCLONEII_M4K_COMPATIBILITY="ON" DEVICE_FAMILY="Cyclone IV E" INDATA_ACLR_A="NONE" LOW_POWER_MODE="AUTO" OPERATION_MODE="DUAL_PORT" OUTDATA_ACLR_B="NONE" OUTDATA_REG_B="UNREGISTERED" RAM_BLOCK_TYPE="AUTO" RDCONTROL_ACLR_B="NONE" RDCONTROL_REG_B="CLOCK0" READ_DURING_WRITE_MODE_MIXED_PORTS="DONT_CARE" WIDTH_A=8 WIDTH_B=8 WIDTH_BYTEENA_A=1 WIDTH_BYTEENA_B=1 WIDTHAD_A=6 WIDTHAD_B=6 WRCONTROL_ACLR_A="NONE" address_a address_b clock0 clock1 clocken1 data_a q_b wren_a CARRY_CHAIN="MANUAL" CARRY_CHAIN_LENGTH=48
--VERSION_BEGIN 13.0 cbx_altsyncram 2013:06:12:18:03:43:SJ cbx_cycloneii 2013:06:12:18:03:43:SJ cbx_lpm_add_sub 2013:06:12:18:03:43:SJ cbx_lpm_compare 2013:06:12:18:03:43:SJ cbx_lpm_decode 2013:06:12:18:03:43:SJ cbx_lpm_mux 2013:06:12:18:03:43:SJ cbx_mgl 2013:06:12:18:05:10:SJ cbx_stratix 2013:06:12:18:03:43:SJ cbx_stratixii 2013:06:12:18:03:43:SJ cbx_stratixiii 2013:06:12:18:03:43:SJ cbx_stratixv 2013:06:12:18:03:43:SJ cbx_util_mgl 2013:06:12:18:03:43:SJ  VERSION_END


-- Copyright (C) 1991-2013 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.


FUNCTION cycloneive_ram_block (clk0, clk1, clr0, clr1, ena0, ena1, ena2, ena3, portaaddr[PORT_A_ADDRESS_WIDTH-1..0], portaaddrstall, portabyteenamasks[PORT_A_BYTE_ENABLE_MASK_WIDTH-1..0], portadatain[PORT_A_DATA_WIDTH-1..0], portare, portawe, portbaddr[PORT_B_ADDRESS_WIDTH-1..0], portbaddrstall, portbbyteenamasks[PORT_B_BYTE_ENABLE_MASK_WIDTH-1..0], portbdatain[PORT_B_DATA_WIDTH-1..0], portbre, portbwe)
WITH ( CLK0_CORE_CLOCK_ENABLE, CLK0_INPUT_CLOCK_ENABLE, CLK0_OUTPUT_CLOCK_ENABLE, CLK1_CORE_CLOCK_ENABLE, CLK1_INPUT_CLOCK_ENABLE, CLK1_OUTPUT_CLOCK_ENABLE, CONNECTIVITY_CHECKING, DATA_INTERLEAVE_OFFSET_IN_BITS, DATA_INTERLEAVE_WIDTH_IN_BITS, DONT_POWER_OPTIMIZE, INIT_FILE, INIT_FILE_LAYOUT, init_file_restructured, LOGICAL_RAM_NAME, mem_init0, mem_init1, mem_init2, mem_init3, mem_init4, MIXED_PORT_FEED_THROUGH_MODE, OPERATION_MODE, PORT_A_ADDRESS_CLEAR, PORT_A_ADDRESS_WIDTH = 1, PORT_A_BYTE_ENABLE_MASK_WIDTH = 1, PORT_A_BYTE_SIZE, PORT_A_DATA_OUT_CLEAR, PORT_A_DATA_OUT_CLOCK, PORT_A_DATA_WIDTH = 1, PORT_A_FIRST_ADDRESS, PORT_A_FIRST_BIT_NUMBER, PORT_A_LAST_ADDRESS, PORT_A_LOGICAL_RAM_DEPTH, PORT_A_LOGICAL_RAM_WIDTH, PORT_A_READ_DURING_WRITE_MODE, PORT_B_ADDRESS_CLEAR, PORT_B_ADDRESS_CLOCK, PORT_B_ADDRESS_WIDTH = 1, PORT_B_BYTE_ENABLE_CLOCK, PORT_B_BYTE_ENABLE_MASK_WIDTH = 1, PORT_B_BYTE_SIZE, PORT_B_DATA_IN_CLOCK, PORT_B_DATA_OUT_CLEAR, PORT_B_DATA_OUT_CLOCK, PORT_B_DATA_WIDTH = 1, PORT_B_FIRST_ADDRESS, PORT_B_FIRST_BIT_NUMBER, PORT_B_LAST_ADDRESS, PORT_B_LOGICAL_RAM_DEPTH, PORT_B_LOGICAL_RAM_WIDTH, PORT_B_READ_DURING_WRITE_MODE, PORT_B_READ_ENABLE_CLOCK, PORT_B_WRITE_ENABLE_CLOCK, POWER_UP_UNINITIALIZED, RAM_BLOCK_TYPE, SAFE_WRITE, WIDTH_ECCSTATUS)
RETURNS ( portadataout[PORT_A_DATA_WIDTH-1..0], portbdataout[PORT_B_DATA_WIDTH-1..0]);

--synthesis_resources = M9K 1 
OPTIONS ALTERA_INTERNAL_OPTION = "OPTIMIZE_POWER_DURING_SYNTHESIS=NORMAL_COMPILATION";

SUBDESIGN altsyncram_r1m1
( 
	address_a[5..0]	:	input;
	address_b[5..0]	:	input;
	clock0	:	input;
	clock1	:	input;
	clocken1	:	input;
	data_a[7..0]	:	input;
	q_b[7..0]	:	output;
	wren_a	:	input;
) 
VARIABLE 
	ram_block2a0 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 0,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 0,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a1 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 1,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 1,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a2 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 2,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 2,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a3 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 3,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 3,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a4 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 4,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 4,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a5 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 5,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 5,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a6 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 6,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 6,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	ram_block2a7 : cycloneive_ram_block
		WITH (
			CLK0_CORE_CLOCK_ENABLE = "ena0",
			CLK0_INPUT_CLOCK_ENABLE = "none",
			CLK1_CORE_CLOCK_ENABLE = "ena1",
			CLK1_INPUT_CLOCK_ENABLE = "ena1",
			CONNECTIVITY_CHECKING = "OFF",
			LOGICAL_RAM_NAME = "ALTSYNCRAM",
			MIXED_PORT_FEED_THROUGH_MODE = "dont_care",
			OPERATION_MODE = "dual_port",
			PORT_A_ADDRESS_WIDTH = 6,
			PORT_A_DATA_WIDTH = 1,
			PORT_A_FIRST_ADDRESS = 0,
			PORT_A_FIRST_BIT_NUMBER = 7,
			PORT_A_LAST_ADDRESS = 63,
			PORT_A_LOGICAL_RAM_DEPTH = 64,
			PORT_A_LOGICAL_RAM_WIDTH = 8,
			PORT_B_ADDRESS_CLEAR = "none",
			PORT_B_ADDRESS_CLOCK = "clock1",
			PORT_B_ADDRESS_WIDTH = 6,
			PORT_B_DATA_OUT_CLEAR = "none",
			PORT_B_DATA_WIDTH = 1,
			PORT_B_FIRST_ADDRESS = 0,
			PORT_B_FIRST_BIT_NUMBER = 7,
			PORT_B_LAST_ADDRESS = 63,
			PORT_B_LOGICAL_RAM_DEPTH = 64,
			PORT_B_LOGICAL_RAM_WIDTH = 8,
			PORT_B_READ_ENABLE_CLOCK = "clock1",
			RAM_BLOCK_TYPE = "AUTO"
		);
	address_a_wire[5..0]	: WIRE;
	address_b_wire[5..0]	: WIRE;

BEGIN 
	ram_block2a[7..0].clk0 = clock0;
	ram_block2a[7..0].clk1 = clock1;
	ram_block2a[7..0].ena0 = wren_a;
	ram_block2a[7..0].ena1 = clocken1;
	ram_block2a[7..0].portaaddr[] = ( address_a_wire[5..0]);
	ram_block2a[0].portadatain[] = ( data_a[0..0]);
	ram_block2a[1].portadatain[] = ( data_a[1..1]);
	ram_block2a[2].portadatain[] = ( data_a[2..2]);
	ram_block2a[3].portadatain[] = ( data_a[3..3]);
	ram_block2a[4].portadatain[] = ( data_a[4..4]);
	ram_block2a[5].portadatain[] = ( data_a[5..5]);
	ram_block2a[6].portadatain[] = ( data_a[6..6]);
	ram_block2a[7].portadatain[] = ( data_a[7..7]);
	ram_block2a[7..0].portawe = wren_a;
	ram_block2a[7..0].portbaddr[] = ( address_b_wire[5..0]);
	ram_block2a[7..0].portbre = B"11111111";
	address_a_wire[] = address_a[];
	address_b_wire[] = address_b[];
	q_b[] = ( ram_block2a[7..0].portbdataout[0..0]);
END;
--VALID FILE
